IoTHub client “C” Library

Revision 1.5

07/02/2015

# Revisions:

|  |  |  |  |
| --- | --- | --- | --- |
| Revision | Updated By | Date | Major updates |
| 0.1 | tameraw | 01/15/2015 | Initial draft |
| 0.2 | tameraw | 01/22/2015 | Reviewed comments and simplified API |
| 0.3 | tameraw | 01/30/2015 | Completed API for both the IOTHUB\_message & IOTHUB\_client |
| 1.0 | tameraw | 03/05/2015 | Updated based on the final implementation of the IOTHUB\_client APIs |
| 1.1 | toercola | 04/14/2015 | Adjust the config to use a function pointer rather than an enum |
| 1.2 | dcristo | 04/19/2015 | Rename DeviceHub to IoTHub |
| 1.3 | Anporumb | 05/18/2015 | Rework to bring \_DoWork and threadlessness. |
| 1.5 | Anporumb | 07/02/2015 | Add \_SetOption |

# Overview

The IoTHub client “C” library offers developers a means of communication to & from an IoTHub.

The library allows a device to achieve the supported communication patterns by a IoT Hub:

* **Event**. A message sent by a device to a IoT Hub. The device does not expect a response from IoT Hub, but the event message can result in errors (e.g. not being processed …).
* **Inquiry**. A message sent by a device to a IoT Hub. The device does expect a response (possibly consisting of multiple messages), and the inquiry can result in errors. (not implemented yet)
* **Notification**. A message sent by IoT Hub to the device. IoT Hub does not expect a response from the device, but the notification can result in errors (e.g. failed delivery…)
* **Command**. A message sent by a IoT Hub to the device. IoT Hub does expect a response (possibly consisting of multiple messages), and the command can result in errors. (not implemented yet)

***Note: Only Event & Notification are available for the spring release.***

***Note: CRUD APIs for IoT Hub are not part of this library (i.e. No APIs in C-library offered for managing a IoT Hub).***

The library offers the following features:

* The library provides an encapsulation for the message transfer between a device & ioTHub. This encapsulates the data and common message properties as defined by section 4.6 in the “[IoT Hub surface](https://microsoft.sharepoint.com/teams/ServiceBus/Shared%20Documents/Device%20Hub/Device%20Hub%20surface%20-%20draft.docx?d=w497a5ec52f6b4f4aa549a624bea7e00b)” document.
* The library supports AMQP and HTTP protocols for communication with a IoT Hub.
* The library uses Proton-C to establish the AMQP communication.
* The output will be a static lib.
* The source code for the library will be available under the “IOTHUB\_client” under the “Azure/azure-iot-client-sdk-for-c” in the GitHub repository.
* The repository is located at: <https://github.com/Azure/azure-iot-client-sdk-for-c.git>

The APIs of this library cannot be called from different threads on the same handle without risking data races. Therefore, should more than 1 thread need to access concurrently the APIs of this module on the same handle, there needs to be a user-level synchronization mechanism that guarantees that two APIs are not called at the same time.

# References

* [Azure IoT Gateway](https://microsoft.sharepoint.com/teams/Azure_IoT/_layouts/15/WopiFrame.aspx?sourcedoc=%7bbb1e2642-9331-4c83-af5a-6db0e081d625%7d&action=view&wdparaid=477A1F25)
* [DeviceHub](https://microsoft.sharepoint.com/teams/ServiceBus/Shared%20Documents/Device%20Hub/devicehub.pptx?d=w48ecd21dc0ad488b85af65fac914bed7)
* [DeviceHub Api Getting Started](https://microsoft.sharepoint.com/teams/ServiceBus/Shared%20Documents/Device%20Hub/DeviceHub%20Api%20Getting%20Started.docx?d=w8dabdec2d9cb4f3386c043b7d17f8831)
* [IoT Hub surface - draft](https://microsoft.sharepoint.com/teams/ServiceBus/Shared%20Documents/Device%20Hub/Device%20Hub%20surface%20-%20draft.docx?d=w497a5ec52f6b4f4aa549a624bea7e00b)
* [IoT Hub Architecture\_revised](https://microsoft.sharepoint.com/teams/ServiceBus/Shared%20Documents/Device%20Hub/Device%20Hub%20Architecture_revised.docx?d=w076021f811a24b87bbfb17493ff87e8a)

# Example1 – SendEventAsync:

#include <stdio.h>

#include <stdlib.h>

#ifdef \_CRTDBG\_MAP\_ALLOC

#include <crtdbg.h>

#endif

#include "gballoc.h"

#include "iothub\_client.h"

#include "iothub\_message.h"

#include "threadapi.h"

#include "crt\_abstractions.h"

#include "iothubtransportamqp.h"

#define MAX\_NUMBER\_OF\_MESSAGES 5

static const unsigned int SLEEP\_IN\_MILLISECONDS = 500;

static const int MESSAGE\_BASE\_TRACKING\_ID = 42;

static int g\_callbackInvoked;

DEFINE\_ENUM\_STRINGS(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT, IOTHUB\_CLIENT\_CONFIRMATION\_RESULT\_VALUES);

DEFINE\_ENUM\_STRINGS(IOTHUB\_CLIENT\_RESULT, IOTHUB\_CLIENT\_RESULT\_VALUES);

typedef struct EVENT\_INSTANCE\_TAG

{

    IOTHUB\_MESSAGE\_HANDLE messageHandle;

    int messageTrackingId;  // For tracking the messages within the user callback.

} EVENT\_INSTANCE;

static void ReceiveConfirmationCallback(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT result, void\* userContextCallback)

{

    EVENT\_INSTANCE\* eventInstance = (EVENT\_INSTANCE\*)userContextCallback;

    (void)printf("Confirmation[%d] received for message tracking id = %d with result = %s\r\n", g\_callbackInvoked, eventInstance->messageTrackingId, ENUM\_TO\_STRING(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT, result));

    /\* Some device specific action code goes here... \*/

    g\_callbackInvoked++;

}

int main(void)

{

    IOTHUB\_CLIENT\_CONFIG iotHubClientConfig;

    IOTHUB\_CLIENT\_HANDLE iotHubClientHandle;

    EVENT\_INSTANCE eventInstance[MAX\_NUMBER\_OF\_MESSAGES];

    size\_t msgLength = 1024;

    const char\* msgText = malloc(msgLength);

    g\_callbackInvoked = 0;

    (void)printf("Starting the IoTHub client sample to Send EVENT Asynchronously...\r\n");

    /\* Setup IoTHub client configuration \*/

    iotHubClientConfig.iotHubName = "sdktesthub";

    iotHubClientConfig.deviceId = "devicec4828b8f55064c8b889be1fd5bf1ae1f";

    iotHubClientConfig.deviceKey = "oUVWpT/yBLl7YuKD324oW+f3ybXgKWLnczg+mamlsT4=";

    iotHubClientConfig.protocol = DeviceClientProvideAmqpResources;

    if ((iotHubClientHandle = IoTHubClient\_Create(&iotHubClientConfig)) == NULL)

    {

        (void)printf("ERROR: iotHubClientHandle is NULL!\r\n");

    }

    else

    {

        for (int i = 0; i < MAX\_NUMBER\_OF\_MESSAGES; i++)

        {

            sprintf\_s((char\*)msgText, msgLength, "Message\_%d\_From\_IoTHubClient", i);

            if ((eventInstance[i].messageHandle = IoTHubMessage\_Create()) == NULL)

            {

                (void)printf("ERROR: IoTHubMessageHandle is NULL!\r\n");

            }

            else

            {

                eventInstance[i].messageTrackingId = MESSAGE\_BASE\_TRACKING\_ID + i;

                if (IoTHubMessage\_SetData(eventInstance[i].messageHandle, (const unsigned char\*)msgText, strlen(msgText)) != IOTHUB\_MESSAGE\_OK)

                {

                    (void)printf("ERROR: IoTHubMessage failed to set data!\r\n");

                }

                else

                {

                    if (IoTHubClient\_SendEVENTAsync(iotHubClientHandle, eventInstance[i].messageHandle, ReceiveConfirmationCallback, &eventInstance[i]) != IOTHUB\_CLIENT\_OK)

                    {

                        (void)printf("ERROR: IoTHubClient\_SendEVENTAsync..........FAILED!\r\n");

                    }

                    else

                    {

                        (void)printf("IoTHubClient\_SendEVENTAsync accepted data for transmission to IoT Hub.\r\n");

while (g\_callbackInvoked < MAX\_NUMBER\_OF\_MESSAGES)

    {

        ThreadAPI\_Sleep(SLEEP\_IN\_MILLISECONDS);

    }

                    }

(void)printf("IoTHubClient\_GetSendStatus() returns %s\r\n", ENUM\_TO\_STRING(IOTHUB\_CLIENT\_RESULT, IoTHubClient\_GetSendStatus( iotHubClientHandle));

                }

            }

        }

    }

    IoTHubClient\_Destroy(iotHubClientHandle);

    return 0;

}

# Example2 – ReceiveNotification

#include <stdio.h>

#include <stdlib.h>

#ifdef \_CRTDBG\_MAP\_ALLOC

#include <crtdbg.h>

#endif

#include "gballoc.h"

#include "IOTHUB\_client.h"

#include "IOTHUB\_message.h"

#include "threadapi.h"

#include "crt\_abstractions.h"

#include "iothubtransportamqp.h"

#define MAX\_NUMBER\_OF\_MESSAGES 100

static const unsigned int SLEEP\_IN\_MILLISECONDS = 500;

static const int MESSAGE\_BASE\_TRACKING\_ID = 42;

static int g\_callbackInvoked;

static int ReceiveNotificationCallback(IOTHUB\_MESSAGE\_HANDLE notificationMessage, void\* userContextCallback)

{

    int\* callbackInvoked = (int\*)userContextCallback;

    const char\* buffer;

    size\_t size;

    IoTHubMessage\_GetData(notificationMessage, (const unsigned char\*\*)&buffer, &size);

    (void)printf("Received Notification [%d] with Data: <<<%.\*s>>> & Size=%d\r\n", \*callbackInvoked, (int)size, buffer, (int)size);

    /\* Some device specific action code goes here... \*/

    (\*callbackInvoked)++;

    IoTHubMessage\_Destroy(notificationMessage);

    return 0;

}

void receivenotificationsample\_run(void)

{

    IOTHUB\_CLIENT\_CONFIG iotHubClientConfig;

    IOTHUB\_CLIENT\_HANDLE iotHubClientHandle;

    g\_callbackInvoked = 0;

    (void)printf("Starting the IoTHub client sample to Receive Notification...\r\n");

    /\* Setup IoTHub client configuration \*/

    iotHubClientConfig.iotHubName = "sdktesthub";

    iotHubClientConfig.deviceId = "devicebc29cd129bcb4494a27ec12f6b560a63";

    iotHubClientConfig.deviceKey = "JD9Ji9alCRLKimKxaaPzw0pEw7E2Cr8JS8Tk7+GkrVY=";

    iotHubClientConfig.protocol = DeviceClientProvideAmqpResources;

    if ((iotHubClientHandle = IoTHubClient\_Create(&iotHubClientConfig)) == NULL)

    {

        (void)printf("ERROR: iotHubClientHandle is NULL!\r\n");

    }

    else

    {

        if (IoTHubClient\_SetNotificationCallback(iotHubClientHandle, ReceiveNotificationCallback, &g\_callbackInvoked) != IOTHUB\_CLIENT\_OK)

        {

            (void)printf("ERROR: IoTHubClient\_SetNotificationCallback..........FAILED!\r\n");

        }

        else

        {

time\_t theTime;

            (void)printf("IoTHubClient\_SetNotificationCallback...successful.\r\n");

while (g\_callbackInvoked < MAX\_NUMBER\_OF\_MESSAGES)

     {

         ThreadAPI\_Sleep(SLEEP\_IN\_MILLISECONDS);

     }

if(IoTHubClient\_GetLastNotificationReceiveTime(iotHubClientHandle, &theTime)!=IOTHUBCLIENT\_OK)

{

printf("unable to provide the last received command time...\r\n");

}

else

{

printf("the time when the last command was received was %s\r\n", ctime(&theTime));

}

        }

    }

    IoTHubClient\_Destroy(iotHubClientHandle);

}

# Types defined by the IoTHub client:

#define IOTHUB\_CLIENT\_RESULT\_VALUES       \

    IOTHUB\_CLIENT\_OK,                     \

    IOTHUB\_CLIENT\_INVALID\_ARG,            \

    IOTHUB\_CLIENT\_ERROR,                  \

    IOTHUB\_CLIENT\_INVALID\_SIZE,           \

    IOTHUB\_CLIENT\_INDEFINITE\_TIME,        \

    IOTHUB\_CLIENT\_SENDSTATUS\_IDLE,        \

    IOTHUB\_CLIENT\_SENDSTATUS\_BUSY         \

DEFINE\_ENUM(IOTHUB\_CLIENT\_RESULT, IOTHUB\_CLIENT\_RESULT\_VALUES);

#define IOTHUB\_CLIENT\_CONFIRMATION\_RESULT\_VALUES     \

    IOTHUB\_CLIENT\_CONFIRMATION\_OK,                   \

IOTHUB\_CLIENT\_CONFIRMATION\_BECAUSE\_DESTROY,      \

    IOTHUB\_CLIENT\_CONFIRMATION\_ERROR                 \

DEFINE\_ENUM(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT, IOTHUB\_CLIENT\_CONFIRMATION\_RESULT\_VALUES);

typedef void\* IOTHUB\_CLIENT\_HANDLE;

typedef void(\*IOTHUB\_CLIENT\_EVENT\_CONFIRMATION\_CALLBACK)(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, IOTHUB\_CLIENT\_CONFIRMATION\_RESULT result, void\* userContextCallback);

typedef int(\*IOTHUB\_CLIENT\_NOTIFICATION\_CALLBACK\_ASYNC)(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, IOTHUB\_MESSAGE\_HANDLE notificationMessage, void\* userContextCallback);

typedef void\*(\*IOTHUB\_CLIENT\_TRANSPORT\_PROVIDER)(void);

typedef struct IOTHUB\_CLIENT\_CONFIG\_TAG

{

    IOTHUB\_CLIENT\_TRANSPORT\_PROVIDER protocol;

    const char\* deviceId;

    const char\* deviceKey;

    const char\* iotHubName;

const char\* iotHubSuffix;

} IOTHUB\_CLIENT\_CONFIG;

# IoTHub client Structures

## IOTHUB\_CLIENT\_CONFIG

### struct members

|  |  |
| --- | --- |
| Name | Description |
| protocol | A function pointer that is passed into the IoTHubClientCreate. A function definition for amqp, DeviceClientProvideAmqpResources, is defined in the include iothubtransportamqp.h. A function definition for http, DeviceClientProvideHttpResources, is defined in the include iothubtransporthttp.h |
| deviceId | A string that identifies the device. |
| deviceKey | The device key used to authenticate the device. |
| iotHubName | The IoT Hub name to which the device is connecting. |
| iotHubSuffix | IoT Hub suffix goes here, e.g., private.azure-devices-int.net. |

# IoTHub client APIs

## Types defined by the IoTHub message module:

#define IOTHUB\_MESSAGE\_RESULT\_VALUES         \

    IOTHUB\_MESSAGE\_OK,                       \

    IOTHUB\_MESSAGE\_INVALID\_ARG,              \

    IOTHUB\_MESSAGE\_ERROR                     \

DEFINE\_ENUM(IOTHUB\_MESSAGE\_RESULT, IOTHUB\_MESSAGE\_RESULT\_VALUES);

typedef void\* IOTHUB\_MESSAGE\_HANDLE;

## IOTHUB\_CLIENT\_HANDLE IoTHubClient\_CreateFromConnectionString(const char\* connectionString, IOTHUB\_CLIENT\_TRANSPORT\_PROVIDER protocol);

Creates a IoT Hub client for communication with an existing IoT Hub using the specified connection string parameter. The API does not allow sharing of a connection across multiple devices. This is a blocking call.

Sample connection string:

HostName=[IoT Hub name goes here].[IoT Hub suffix goes here, e.g., private.azure-devices-int.net]; CredentialScope=Device;DeviceId= [Device ID goes here];SharedAccessKey= [Device key goes here];

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| connectionString | Pointer to a character string |
| protocol | Function pointer for protocol implementation |

### Return

* A None-NULL handle value that is used when invoking other functions for IoT Hub client.
* NULL on failure.

typedef void\* IOTHUB\_MESSAGE\_HANDLE;

## IOTHUB\_CLIENT\_HANDLE IoTHubClient\_Create(const IOTHUB\_CLIENT\_CONFIG\* config);

Creates a IoT Hub client for communication with an existing IoT Hub using the specified parameters. The API does not allow sharing of a connection across multiple devices. This is a blocking call.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| config | Pointer to a IOTHUB\_CLIENT\_CONFIG structure |

### Return

* A None-NULL handle value that is used when invoking other functions for IoT Hub client.
* NULL on failure.

## void IoTHubClient\_Destroy(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle);

Disposes of resources allocated by the IoT Hub client. This is a blocking call.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |

### Return

* No return.

## extern IOTHUB\_CLIENT\_RESULT IoTHubClient\_SendEventAsync(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, IOTHUB\_MESSAGE\_HANDLE eventMessageHandle, IOTHUB\_CLIENT\_EVENT\_CONFIRMATION\_CALLBACK eventConfirmationCallback, void\* userContextCallback);

Asynchronous call to send the message specified by the IoTHubMessageHandle.

**NOTE: The application behavior is undefined if the user calls the IoTHubClient\_Destroy from within any callback.**

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |
| eventMessageHandle | The handle to a IoT Hub message. |
| eventConfirmationCallBack | The callback specified by the device for receiving confirmation of the delivery of the IoT Hub message. This callback can be expected to invoke the SendAsync for the same message in attempt to retry sending a failing message. The user can specify a NULL value here to indicate no callback required. |
| userContextCallback | User specified context that will be provided to the callback. This can be NULL. |

### Return

* IOTHUB\_CLIENT\_OK upon success.
* Error code upon failure.

## IOTHUB\_CLIENT\_RESULT IoTHubClient\_SetNotificationCallback(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, IOTHUB\_CLIENT\_NOTIFICATION\_CALLBACK\_ASYNC notificationCallback, void\* userContextCallback);

Sets up the notification callback invoked when IoT Hub issues a notification to the device. This is a blocking call. **NOTE: The application behavior is undefined if the user calls the IoTHubClient\_Destroy from within any callback.**

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |
| notificationCallback | The callback specified by the device for receiving notification messages from IoT Hub. |
| userContextCallback | User specified context that will be provided to the callback. This can be NULL. |

### Return

* IOTHUB\_CLIENT\_OK upon success.
* Error code upon failure.

## IOTHUB\_CLIENT\_RESULT IoTHubClient\_GetLastNotificationReceiveTime (IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, time\_t\* lastNotificationReceiveTime);

This function returns in the out parameter lastNotificationReceiveTime what was the value of the time() function when the last notification was received at the client.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |
| lastNotificationReceiveTime | Out parameter containing the value of time() function when the last notification was received |

### Return

* IOTHUB\_CLIENT\_OK upon success.
* Error code upon failure.

## IOTHUB\_CLIENT\_RESULT IoTHubClient\_GetSendStatus (IOTHUB\_CLIENT\_HANDLE iotHubClientHandle);

This function returns the current sending status for IoTHubClient**.**

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |

### Return

* IOTHUBCLIENT \_INVALID\_ARG if called with NULL parameter
* IOTHUBCLIENT\_SENDSTATUS\_IDLE if there is currently no items to be send
* IOTHUBCLIENT\_SENDSTATUS\_BUSY if there are currently items to be send

## IOTHUB\_CLIENT\_NOTIFICATION\_CALLBACK\_ASYNC

Once a notification is received from the service, if the user has set a call back, the receive callback shall be invoked.

This call back is defined as:

typedef int(\*IOTHUB\_CLIENT\_NOTIFICATION\_CALLBACK\_ASYNC)(IOTHUB\_MESSAGE\_HANDLE notificationMessage, void\* userContextCallback);

If the user returns from the call back the status 0, IOTHUB\_Cliend will accept the notification, meaning that it will not be received again by the client. If the user returnas a non-Zero Value, the notification will be rejected. notificationMessage is only valid in the scope of the callback.

## IOTHUB\_CLIENT\_RESULT IoTHubClient\_SetOption(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle, const char\* optionName, const void\* value);

IoTHubClient\_SetOption shall set a runtime option identified by parameter "optionName" to a value pointed to by parameter value. The optionName and the data type value is pointing to are specific for every option.

Options:

"timeout" - the maximum time in miliseconds a communication is allowed to use. value is a pointer to an unsigned int with the meaning of "miliseconds". This is only supported for HTTP protocol so far. When the HTTP protocol uses CURL, the meaning of the parameter is total request time. When the HTTP protocol uses winhttp, the meaning is dwSendTimeout and dwReceiveTimeout parameters of [WinHttpSetTimeouts](https://msdn.microsoft.com/en-us/library/windows/desktop/aa384116(v=vs.85).aspx) API.

"[CURLOPT\_LOW\_SPEED\_LIMIT](http://curl.haxx.se/libcurl/c/CURLOPT_LOW_SPEED_LIMIT.html)" - only available for HTTP protocol and only when CURL is used. It has the same meaning as CURL's option with the same name. value is pointer to a long.

"[CURLOPT\_LOW\_SPEED\_TIME](http://curl.haxx.se/libcurl/c/CURLOPT_LOW_SPEED_TIME.html)" - only available for HTTP protocol and only when CURL is used. It has the same meaning as CURL's option with the same name. value is pointer to a long.

"[CURLOPT\_FORBID\_REUSE](http://curl.haxx.se/libcurl/c/CURLOPT_FORBID_REUSE.html)" - only available for HTTP protocol and only when CURL is used. It has the same meaning as CURL's option with the same name. value is pointer to a long.

"[CURLOPT\_FRESH\_CONNECT](http://curl.haxx.se/libcurl/c/CURLOPT_FRESH_CONNECT.html)" - only available for HTTP protocol and only when CURL is used. It has the same meaning as CURL's option with the same name. value is pointer to a long.

"[CURLOPT\_VERBOSE](http://curl.haxx.se/libcurl/c/CURLOPT_VERBOSE.html)" - only available for HTTP protocol and only when CURL is used. It has the same meaning as CURL's option with the same name. value is pointer to a long.

## IotHubClient\_LL\_... APIs

IoTHubClient API surface also contains a separate set of APIs that allow the user to interact with the lower layer portion of the IoTHubClient. These APIs contain \_LL\_ in their name, but retain the same functionality like the IoTHubClient\_... APIs, with one difference. If the \_LL\_ APIs are used the user is responsible for scheduling when the actual work done by the IoTHubClient happens (when the data is sent/received on/from the wire). This is useful for constrained devices where spinning a separate thread is often not desired.

## IOTHUB\_CLIENT\_RESULT void IoTHubClient\_LL\_DoWork(IOTHUB\_CLIENT\_HANDLE iotHubClientHandle);

This function is user called when work (sending/receiving) can be done by the IoTHubClient**.** All IoTHubClient interactions (in regards to network trafic and/or user level callbacks) are the effect of calling this function and they take place synchronously inside \_DoWork.

Arguments:

|  |  |
| --- | --- |
| Name | Description |
| iotHubClientHandle | The handle created by a call to the create function. |

Example of using DoWork:

#include <stdio.h>

#include <stdlib.h>

#ifdef \_CRTDBG\_MAP\_ALLOC

#include <crtdbg.h>

#endif

#include "gballoc.h"

#include "iothub\_client.h"

#include "iothub\_message.h"

#include "threadapi.h"

#include "crt\_abstractions.h"

#include "iothubtransportamqp.h"

#define MAX\_NUMBER\_OF\_MESSAGES 5

static const unsigned int SLEEP\_IN\_MILLISECONDS = 500;

static const int MESSAGE\_BASE\_TRACKING\_ID = 42;

static int g\_callbackInvoked;

DEFINE\_ENUM\_STRINGS(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT, IOTHUB\_CLIENT\_CONFIRMATION\_RESULT\_VALUES);

DEFINE\_ENUM\_STRINGS(IOTHUB\_CLIENT\_RESULT, IOTHUB\_CLIENT\_RESULT\_VALUES);

typedef struct EVENT\_INSTANCE\_TAG

{

    IOTHUB\_MESSAGE\_HANDLE messageHandle;

    int messageTrackingId;  // For tracking the messages within the user callback.

} EVENT\_INSTANCE;

static void ReceiveConfirmationCallback(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT result, void\* userContextCallback)

{

    EVENT\_INSTANCE\* eventInstance = (EVENT\_INSTANCE\*)userContextCallback;

    (void)printf("Confirmation[%d] received for message tracking id = %d with result = %s\r\n", g\_callbackInvoked, eventInstance->messageTrackingId, ENUM\_TO\_STRING(IOTHUB\_CLIENT\_CONFIRMATION\_RESULT, result));

    /\* Some device specific action code goes here... \*/

    g\_callbackInvoked++;

}

int main(void)

{

    IOTHUB\_CLIENT\_CONFIG iotHubClientConfig;

    IOTHUB\_CLIENT\_HANDLE iotHubClientHandle;

    EVENT\_INSTANCE eventInstance[MAX\_NUMBER\_OF\_MESSAGES];

    size\_t msgLength = 1024;

    const char\* msgText = malloc(msgLength);

    g\_callbackInvoked = 0;

    (void)printf("Starting the IoTHub client sample to Send Event Asynchronously...\r\n");

    /\* Setup IoTHub client configuration \*/

    iotHubClientConfig.iotHubName = "sdktesthub";

    iotHubClientConfig.deviceId = "devicec4828b8f55064c8b889be1fd5bf1ae1f";

    iotHubClientConfig.deviceKey = "oUVWpT/yBLl7YuKD324oW+f3ybXgKWLnczg+mamlsT4=";

iotHubClientConfig.iotHubSuffix = "private.azure-devices-int.net";

    iotHubClientConfig.protocol = DeviceClientProvideAmqpResources;

    if ((iotHubClientHandle = IoTHubClient\_LL\_Create(&iotHubClientConfig)) == NULL)

    {

        (void)printf("ERROR: iotHubClientHandle is NULL!\r\n");

    }

    else

    {

        for (int i = 0; i < MAX\_NUMBER\_OF\_MESSAGES; i++)

        {

            sprintf\_s((char\*)msgText, msgLength, "Message\_%d\_From\_IoTHubClient", i);

            if ((eventInstance[i].messageHandle = IoTHubMessage\_Create()) == NULL)

            {

                (void)printf("ERROR: IoTHubMessageHandle is NULL!\r\n");

            }

            else

            {

                eventInstance[i].messageTrackingId = MESSAGE\_BASE\_TRACKING\_ID + i;

                if (IoTHubMessage\_SetData(eventInstance[i].messageHandle, (const unsigned char\*)msgText, strlen(msgText)) != IOTHUB\_MESSAGE\_OK)

                {

                    (void)printf("ERROR: IoTHubMessage failed to set data!\r\n");

                }

                else

                {

                    if (IoTHubClient\_LL\_SendEventAsync(iotHubClientHandle, eventInstance[i].messageHandle, ReceiveConfirmationCallback, &eventInstance[i]) != IOTHUB\_CLIENT\_OK)

                    {

                        (void)printf("ERROR: IoTHubClient\_LL\_SendEventAsync..........FAILED!\r\n");

                    }

                    else

                    {

                        (void)printf("IoTHubClient\_LL\_SendEventAsync accepted data for transmission to IoT Hub.\r\n");

while (g\_callbackInvoked < MAX\_NUMBER\_OF\_MESSAGES)

    {

IoTHubClient\_LL\_DoWork(iotHubClientHandle);

        ThreadAPI\_Sleep(SLEEP\_IN\_MILLISECONDS);

    }

                    }

(void)printf("IoTHubClient\_GetSendStatus() returns %s\r\n", ENUM\_TO\_STRING(IOTHUB\_CLIENT\_RESULT, IoTHubClient\_GetSendStatus( iotHubClientHandle));

                }

            }

        }

    }

    IoTHubClient\_LL\_Destroy(iotHubClientHandle);

    return 0;

}

# IoTHub message APIs

## IOTHUB\_MESSAGE\_HANDLE IoTHubMessage\_Create(void);

Creates an empty IoT Hub message to be used for operations between the device and IoT Hub.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| void |  |

### Return

* A None-NULL handle value that is used when invoking other functions for IoT Hub message.
* NULL on failure.

## void IoTHubMessage\_Destroy(IOTHUB\_MESSAGE\_HANDLE ioTHubMessageHandle);

Disposes of resources allocated by the IoT Hub message.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| ioTHubMessageHandle | The handle created by a call to the create function. |

### Return

* No return.

## IOTHUB\_MESSAGE\_RESULT IoTHubMessage\_SetData(IOTHUB\_MESSAGE\_HANDLE ioTHubMessageHandle, const unsigned char\* buffer, size\_t size);

Allocates memory and sets the data for the specified device message handle. This API will make a copy of the buffer input.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| ioTHubMessageHandle | The handle created by a call to the create function. |
| buffer | A pointer to the data |
| size | Specifies the size of the data in bytes |

### Return

* IOTHUB\_MESSAGE\_OK upon success.
* Error code upon failure.

## IOTHUB\_MESSAGE\_RESULT IoTHubMessage\_GetData(IOTHUB\_MESSAGE\_HANDLE ioTHubMessageHandle, const unsigned char\*\* buffer, size\_t\* size);

Provides the data and size associated with a IoTHubMessageHandle.

### Arguments

|  |  |
| --- | --- |
| Name | Description |
| ioTHubMessageHandle | The handle created by a call to the create function. |
| buffer | Output parameter for the data. |
| size | Output parameter for the length of the data buffer |

### Return

* IOTHUB\_MESSAGE\_OK upon success.
* Error code upon failure.